1. Default baud rate is 115200, N, 8, 1.

2. module contains tow MAC address, 00:0E:0B:xx:xx:xx is BLE mode, 00:0E:0E:xx:xx:xx is EDR mode.

3. Our company provides two version bluetooth serial assistant, BLE Comassistant and SPP ComAssistant.

4. Dont iperate the BLE in android Bluetooth management interface.

5. Before V216 PIO0 must be pull up.

6. Since V216 you can shut down PIO0 function use "AT+PIO0" command. After execute "AT+PIO00" command, you can left PIO0 NC.

7. Since V216 we setup "AT+PIO00" as default settings.

8. Query version command is "AT+VERS?"

9. The AT command is uppercase characters, dont have any other symbols.

A. Dual mode module dont have high speed, Please make some delay time between two packages.


