jnhuamao technology co,. ltd.

www.jnhuamao.cn

-------------------------------------------------------------------------------
-------------------------------------------------------------------------------

CC2540 Bluetooth Low Energy USB Dongle Firmware
Release Notes

-------------------------------------------------------------------------------
-------------------------------------------------------------------------------
Version 526
2015-04-28

Notices:

- Add some AT commands.
- Change some workflow of discovery.
  
Changes and Enhancements:

1. Add AT+COMI command, config Minimum Link Layer connection interval
   para1 value: 0 ~ 9; Default: 3(20ms);
   0: 7.5ms; 1: 10ms; 2: 15ms; 3: 20ms; 4: 25ms; 5: 30ms; 6: 35ms; 7: 40ms; 8: 45ms; 9: 4000ms
2. Add AT+COMA command, config Maximum Link Layer connection interval
   para1 value: 0 ~ 9; Default: 7(40ms);
   0: 7.5ms; 1: 10ms; 2: 15ms; 3: 20ms; 4: 25ms; 5: 30ms; 6: 35ms; 7: 40ms; 8: 45ms; 9: 4000ms
3. Add AT+COLA command, config Link Layer connection slave latency
   para1 value: 0 ~ 4; Default: 0;
4. Add AT+COSU command, config Link Layer connection supervision timeout
   para1 value: 0 ~ 6; Default: 6(6000ms);
   0: 100ms; 1: 1000ms; 2: 2000ms; 3: 3000ms; 4: 4000ms; 5: 5000ms; 6: 6000ms;
5. Add AT+COUP command, switch slave role update connection parameter
   para1 value 0, 1; Default: 1(Update on);
   0: Update off; 1: Update on;
6. Add AT+GAIN command, setup RX gain
   para1 value: 0~1


Version 525
2014-12-01

Notices:

- Fix some bugs.
- Add some AT commands.
- Change some workflow of discovery.
  
Changes and Enhancements:

- Add AT+NOTP command (switch promte string format)


Version 513
2013-12-13

Notices:

- Fix some bugs.
- Add some AT commands.
- Change some workflow of discovery.
  
Changes and Enhancements:

- Add AT+IBEA command (Open close iBeacon)
- Add AT+MARJ command (Query/Set iBeacon marjor)
- Add AT+MINO command (Query/Set iBeacon minor)

-------------------------------------------------------------------------------
-------------------------------------------------------------------------------

